`

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change Status** | | | | | | | |
| Issue Date | Version | | Summary | | | | Remark |
| 2020-03-18 | A0 | | Document Issue | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
| Approved By | | | Checked By | | Prepared By | | |
|  | | |  | |  | | |
| Copy File Department Distribution Detail | | | | | | | |
| Quality Dept. | |  | | SD | |  | |
| Pur. Dept. | |  | |  | |  | |
| Engineering Dept. | |  | |  | |  | |
| MD | |  | |  | |  | |
| This document is stamped with the issuing and issuing date. | | | | | | | |

1. Purchase: In order to declare the TPD demand
2. Function: The document is prepared by the market department.


3、Detail Content :

a) Opening System: Refill the e-liquid from the top of atomizer (The top cap with atomizer head).

b) Operation instructions: Screw off the top cap and Refill the e-liquid from the hole on the top. The e-liquid capacity is 5.0 ml.

c) Note: Please don’t overfill when reassemble.

d) Filling Structure



e) Application of Product: Obelisk 120 FC Kit.